|  |  |  |
| --- | --- | --- |
| TC – 6C EP CLAW LOCK POINTS OPERATING TEST CERTIFICATE | No. |       |

|  |  |
| --- | --- |
| **Please make a selection:** | [ ]  IN-BEARER / [ ]  ON-BEARER\*\* |
| [ ]  CONCRETE / [ ]  TIMBER / [ ]  STEEL\*\* / [ ]  FFU / [ ]  Other\*\* |

|  |
| --- |
|       |

 |

|  |  |  |
| --- | --- | --- |
| **LOCATION:** |       | Tests to be carried out in accordance with PR S 40030, Manual TMG E1341 & TMG E1343 |
| **PROJECT:** |       |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **POINT END** | **STYLE\***Select from:**A****S****E****ES****T** | **SWITCH OPENING***Tangential**125 -140mm60kg 125-130mm53kg 110-115mm*(mm) | **LOCK SET DIMENSION***Trailable**0 to -10mm**Non-trailable ±10mm*(mm) | **FLANGEWAY CLEARANCE**FEG TEST(where T crank backdrives are fitted)ORRear Flange OpeningMinimum 60mm*at narrowest point* | **POINT LOCK TEST***Go 3.2mmNo-Go 4.8mm*(✓ when correct) | **CLAW LOCK COVERAGE** (EP Points)*Min 20mm point lock coverage with* ***open switch detector*** *contacts made*(mm) | **OPERATING BAR DETECTION TEST**(Catchpoints & Independent Switches)*Min 30mm point lock coverage with operating bar detector contacts made*(mm) | **PNEUMATIC MOTOR DETECTION TEST**(where fitted)*Min 30mm point lock coverage with motor switch contacts made*(mm) | **POINT SWITCH DETECTION TEST***‘just made’ 3.2mm‘visibly open’ 4.8mm****+ see note below***(✓ when correct) | **CORRESPONDENCE TEST*includes Out of Correspondence****refer to SPG 0711.4 for test combinations*(✓ when complete) | **PRESSURE SWITCH DETECTION**(✓ when correct) |
| **LHSC** | **RHSC** | **LHSC** | **RHSC** | **LHSC** | **RHSC** | **NOR** | **REV** | **NOR** | **REV** | **Closed Switch** | **NOR** | **REV** | **NOR** | **REV** | **NOR** | **REV** |
|       |       |       |       |       |       | [ ]   |       | [ ]   |       | [ ]   | [ ]   |       |       |       |       |       | [ ]   | [ ]   | [ ]   | [ ]   | [ ]   |
|       |       |       |       |       |       | [ ]   |       | [ ]   |       | [ ]   | [ ]   |       |       |       |       |       | [ ]   | [ ]   | [ ]   | [ ]   | [ ]   |
|       |       |       |       |       |       | [ ]   |       | [ ]   |       | [ ]   | [ ]   |       |       |       |       |       | [ ]   | [ ]   | [ ]   | [ ]   | [ ]   |
|       |       |       |       |       |       | [ ]   |       | [ ]   |       | [ ]   | [ ]   |       |       |       |       |       | [ ]   | [ ]   | [ ]   | [ ]   | [ ]   |
| **REMARKS:** Point History Card complete [ ]   | **Lock Set Dimensions** |
|       |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **TESTER’S NAME:** |       | **SIGNATURE:** |  | **DATE:** |       |
| **Received/Checked/Actioned by NAME:** |       | **SIGNATURE:** |  | **DATE:** |       |

**NOTES:**

\* (CONTROL VALVE) STYLE: **A / S / E / ES / T**

\*\* Please ✓ applicable

+ Set-up detector slides with 3.2mm and 4.8mm gauges no more than 75mm from the tip. Final certification detection testing is to be carried out using 1mm ‘go’ and 2mm ‘no-go’ gauges. Confirm that the detector contacts tested are actuated by the detector rod connected to the closed switch. Ensure the contacts actually open when the detector roller has reached a position along the slide notch that should activate the contact block.