|  |  |  |
| --- | --- | --- |
| TC – 6C EP CLAW LOCK POINTS OPERATING TEST CERTIFICATE | No. |  |

|  |  |  |
| --- | --- | --- |
| **Please make a selection:** | IN-BEARER /  ON-BEARER\*\* | |
| CONCRETE /  TIMBER /  STEEL\*\* /  FFU /  Other\*\* | |  | | --- | |  | |

|  |  |  |
| --- | --- | --- |
| **LOCATION:** |  | Tests to be carried out in accordance with PR S 40030, Manual TMG E1341 & TMG E1343 |
| **PROJECT:** |  | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **POINT END** | **STYLE\***  Select from:  **A**  **S**  **E**  **ES**  **T** | **SWITCH OPENING**  *Tangential*  *125 -140mm 60kg 125-130mm 53kg 110-115mm*  (mm) | | **LOCK SET DIMENSION**  *Trailable*  *0 to -10mm*  *Non-trailable ±10mm*  (mm) | | **FLANGEWAY CLEARANCE**  FEG TEST(where T crank backdrives are fitted)  OR  Rear Flange Opening  Minimum 60mm  *at narrowest point* | | | | **POINT LOCK TEST**  *Go 3.2mm No-Go 4.8mm*  (✓ when correct) | | **CLAW LOCK COVERAGE**  (EP Points)  *Min 20mm point lock coverage with* ***open switch detector*** *contacts made*  (mm) | | **OPERATING BAR DETECTION TEST** (Catchpoints & Independent Switches)  *Min 30mm point lock coverage with operating bar detector contacts made*  (mm) | **PNEUMATIC MOTOR DETECTION TEST** (where fitted)  *Min 30mm point lock coverage with motor switch contacts made*  (mm) | | **POINT SWITCH DETECTION TEST**  *‘just made’ 3.2mm ‘visibly open’ 4.8mm*  ***+ see note below***  (✓ when correct) | | **CORRESPONDENCE TEST *includes Out of Correspondence*** *refer to SPG 0711.4 for test combinations*  (✓ when complete) | **PRESSURE SWITCH DETECTION**  (✓ when correct) | |
| **LHSC** | **RHSC** | **LHSC** | **RHSC** | **LHSC** | | **RHSC** | | **NOR** | **REV** | **NOR** | **REV** | **Closed Switch** | **NOR** | **REV** | **NOR** | **REV** | **NOR** | **REV** |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **REMARKS:** Point History Card complete | | | | | | | | | | | **Lock Set Dimensions** | | | | | | | | | | |
|  | | | | | | | | | | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **TESTER’S NAME:** |  | | **SIGNATURE:** |  | **DATE:** |  |
| **Received/Checked/Actioned by NAME:** | |  | **SIGNATURE:** |  | **DATE:** |  |

**NOTES:**

\* (CONTROL VALVE) STYLE: **A / S / E / ES / T**

\*\* Please ✓ applicable

+ Set-up detector slides with 3.2mm and 4.8mm gauges no more than 75mm from the tip. Final certification detection testing is to be carried out using 1mm ‘go’ and 2mm ‘no-go’ gauges. Confirm that the detector contacts tested are actuated by the detector rod connected to the closed switch. Ensure the contacts actually open when the detector roller has reached a position along the slide notch that should activate the contact block.