|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Track****Sections** |  | **Wheel Sensor Name** |  | **Wheel Sensor** **ID** |  | **Location** |  | **SV Section(s)****(Y/N)** |  | **Counting Head Cont.****(Y/N)** |  |
| **Date** | **Remarks – Fault or Service Schedule** (F, SS01, SS02 etc.) | **Wheel Sensor** | **Calibration**(mV) | **Test Value** (mV) | **Assignment Check** | **Vertical Position (mm)** | **Horizontal Position (mm)** | **Occupancy Det'neach T/Section (OK/NA)** | **Comments**(e.g. Meter Type & Serial No./ASD Cable, Reset)  | **Name** |
| **Serial Number** | Sys1  | Sys2  | Sys1\*¹ | Sys2\*¹ |
|  | First full recorded test |  |  |  |  |  |  |  |  |  |  |  |
|  | Last full recorded test |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
| \*¹ - Check and record that the Axle Counter Wheel Sensor (Systems 1 and 2) are within 95 - 107% of calibration value and 20mV of each other – recalibrate if outside of these values. |
| **Date** | **Remarks – Fault or Service Schedule** (F, SS01, SS02 etc.) | **Wheel Sensor** | **Calibration**(mV) | **Test Value** (mV) | **Assignment Check** | **Vertical Position (mm)** | **Horizontal Position (mm)** | **Occupancy Det'neach T/Section (OK/NA)** | **Comments**(e.g. Meter Type & Serial No./ASD Cable, Reset)  | **Name** |
| **Serial Number** | Sys1  | Sys2  | Sys1\*¹ | Sys2\*¹ |
|  | First full recorded test |  |  |  |  |  |  |  |  |  |  |  |
|  | Last full recorded test |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
| \*¹ - Check and record that the Axle Counter Wheel Sensor (Systems 1 and 2) are within 95 - 107% of calibration value and 20mV of each other – recalibrate if outside of these values. |