|  |  |  |
| --- | --- | --- |
|  | Certificate No. |  |
| *Testing shall be conducted in accordance with the following reference documents:**PR S 40030 Point Lock and Detection Testing on Power Operated Points**PR S 47114 Inspection and Testing of Signalling: Inspection and Testing Procedures**MN S 41581 Electric Point Machine M3A Mk2**MN S 41582 Electric Point Machine Nippon KA1211 B and C**MN S 41584 Electric Point Machine GEC type HW**MN S 41292 Backdrives Setup, Adjustment and Maintenance* |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Project: |  | Location: |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| POINT END | MACHINE1 | BEARER TYPE1 | TURNOUT TYPE1 | BACKDRIVE1 | SWITCH OPENING (mm) | FLANGEWAY CLEARANCE3 | POINT LOCK4 | SWITCH DETECTION4 | LOCK PROVING4 | CORRESPONDENCE/ OUT OF CORRESPONDENCE TEST4 | MOTOR OPERATION | POINT HISTORY CARD COMPLETED4 |
| SIEMENS M3A | NIPPON KA1211 | GEC HW4400 | OTHER2 | CONCRETE | TIMBER | FFU | OTHER2 | 60kg TANG. | 60kg CONV. | 53kg CONV. | T CRANK | OTHER2 | NONE | OPERATING VOLTAGE (V) | OPERATING CURRENT (A) | CLUTCH SLIP CURRENT (A) | OPERATING TIME (s) | CUT-OUT TIME (s) |
| LH | RH | LH | RH | LH | RH | LH | RH | LH | RH |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 1. TICK WHERE APPLICABLE.
2. PROVIDE DETAILS IN NOTES.
3. TEST WITH FEG WHERE BACKDRIVE FITTED, OTHERWISE 60mm MINIMUM OPENING AT NARROWEST POINT. TICK WHERE CORRECT.
4. TICK WHERE CORRECT.
 |

|  |
| --- |
| NOTES/REMARKS: |

|  |
| --- |
| **TESTER** |
| NAME: |  | SIGNATURE: |  | DATE: |  |
| **RECEIVED/CHECKED/ACTIONED BY** |
| NAME: |  | SIGNATURE: |  | DATE: |  |