 **Licence No 4627 - Publication of Monitoring Data M8 St Peters Interchange – 10-16 Albert Street, St Peters**

**Disclaimer:** *In NSW, section 66(6) of the Protection of the Environment Operations Act 1997 (****POEO Act****) requires holders of environment protection licences to make their pollution monitoring data publicly available. Accordingly, the monitoring data below is provided to meet Transport for NSW (****TfNSW****) obligations under section 66(6) the POEO Act and any associated guidance documentation published by the Environment Protection Authority (*[*www.epa.nsw.gov.au*](http://www.epa.nsw.gov.au)*). TfNSW recognises that the intent of section 66(6) of the POEO Act is to improve the general public’s access to information about the environmental performance of licensed facilities. To the best of TfNSW’s knowledge, the data contained in this document is as accurate as possible. No material in this document is to be reproduced or published elsewhere in any form without TfNSW’s prior written consent.*

*Link to licence on EPA website;*

[**https://app.epa.nsw.gov.au/prpoeoapp/ViewPOEOLicence.aspx?DOCID=194233&SYSUID=1&LICID=4627**](https://app.epa.nsw.gov.au/prpoeoapp/ViewPOEOLicence.aspx?DOCID=194233&SYSUID=1&LICID=4627)

**Ambient Monitoring – Air Quality**

**EPL No: 4627**

**Date of Sampling 24/09/2023 – 26/10/23**

**Date of Publication 27 February 2024**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Sampling point | Monitoring frequency required by licence | Pollutant | Measurement | Unit |
| DM01 | Monthly | Total suspended particles | 2.2 | Grams per square metre per month |

NOTES:

EPL - Environment Protection Licence

Sample point CPB - DM01 - Dust deposition bottle placed adjacent to minor remediation works at Bridge 5

*The goal is 4g/m²/month on a 12 month moving average.*

*For Sampling Point DM01 the 12 month moving average will be included when results for a 12 month period are available.*